

   "HereticaL" musicdisk...


For some historical knowledge read the HRTCL.NFO file...


The lowest configuration we could test the disk on was a P120 with S3Trio64
and 16meg RAM and it runs just fine... I cannot say it would be smooth
on 486's but it is supposed to be anyway...

A DPMI server is needed... The PMODE/DJ extender is buggy (at least the
version which we use) that lock-ups expected on DOS configurations with
no memory managers at all...

For low level graphics operations the Allegro lib from Shawn Hargreaves
was used... The lib supports VESA 1.x, 2.x and native SVGA drivers... First
VESA 2.x is detected and used so if you have a buggy VESA driver (such as
ViRGE internal VBE2.0 driver) you can force the disk to use S3 native
driver via commandline parameter '-s3'.. VESA 2.0 is the fastest however...

You shouldn't have any sound problems.. If you have, then check your
BLASTER or ULTRASND settings... The sound code wasn't tested with GUS
cards and we don't know if it will work but we trust MikMod coders anyway :)

mikmod/DJ v2.10 used.. The DMA code for DJGPP was buggy and I'd patched it so
there should be no problems...

If you have comments:

  ssg@ogu.edu.tr

