WROTKI#6 DOC FILE.

i)  po polsku
ii) in english

i) po polsku:

1. Na GUSie Wrotki#6 nie dzia’aj† na przerwaniu wi‘kszym ni§ 7
   (na 7 dzia’a).
2. Ustawienie wyjžcia d¦wi‘ku na 16-bit˘w lub jego jakožci
   na wi‘ksz† ni§ Very Low na komputerze z procesorem
   s’abszym ni§ P100 mo§e powodowaŤ bardzo wolne dzia’anie
   programu.
   Kod zosta’ przetestowany na wielu konfiguracjach sprz‘towych.
   Przyk’adowa proponowana konfiguracja:

   Procesor:             Wyjžcie d¦wi‘ku:      JakožŤ d¦wi‘ku:
   486DX (80 Mhz)        8-bit mono            Very Low
   5x86 P75 (133 Mhz)    8-bit stereo          Very Low
                         (ew.16-bit mono)
   P133                  16-bit stereo         Low
   P200                  16-bit stereo         Medium

ii) in english:

1. On GUS Wrotki#6 doesn't work on IRQ higher than 7
   (it works on IRQ 7).
2. Setting the 16-bit output mode or sound quality
   higher than Very Low can cause Wrotki#6 to run
   very slow on something under P100.
   Code was tested on many hardware configurations.
   Sample configuration:

   Procesor:             Output mode:          Sound quality:
   486DX (80 Mhz)        8-bit mono            Very Low
   5x86 P75 (133 Mhz)    8-bit stereo          Very Low
                         (or 16-bit mono)
   P133                  16-bit stereo         Low
   P200                  16-bit stereo         Medium

<file end