K„ytt”j„rjestelm„n kuulu olla D-O-S, jos toimivuus on takeena!
Koneena sais olla P100 ainaki...
Muistia tarvii olla noin 520kB basea, ja viel„ noin 500kiloo
jotain muuta muistia muusiikille!


Modules using memory below 1 MB:

  Name           Total           Conventional       Upper Memory
  --------  ----------------   ----------------   ----------------
  SYSTEM      18,688   (18K)     12,688   (12K)      6,000    (6K)
  HIMEM       35,184   (34K)     35,184   (34K)          0    (0K)
  EMM386       3,120    (3K)      3,120    (3K)          0    (0K)
  4DOS         4,016    (4K)      4,016    (4K)          0    (0K)
  SMARTDRV    29,040   (28K)     12,640   (12K)     16,400   (16K)
  GMOUSE      18,704   (18K)     18,432   (18K)        272    (0K)
  CTSB16      26,816   (26K)          0    (0K)     26,816   (26K)
  CTMMSYS     10,544   (10K)          0    (0K)     10,544   (10K)
  IFSHLP       2,864    (3K)          0    (0K)      2,864    (3K)
  SETVER         832    (1K)          0    (0K)        832    (1K)
  KEYB         6,944    (7K)          0    (0K)      6,944    (7K)
  Free       591,456  (578K)    569,040  (556K)     22,416   (22K)

Memory Summary:

  Type of Memory       Total         Used          Free
  ----------------  -----------   -----------   -----------
  Conventional          655,360        86,320       569,040
  Upper                  93,088        70,672        22,416
  Reserved              393,216       393,216             0
  Extended (XMS)*    32,412,768     2,643,040    29,769,728
  ----------------  -----------   -----------   -----------
  Total memory       33,554,432     3,193,248    30,361,184

  Total under 1 MB      748,448       156,992       591,456

  Total Expanded (EMS)                 32,817,152    (31M)
  Free Expanded (EMS)*                 29,868,032    (28M)

  * EMM386 is using XMS memory to simulate EMS memory as needed.
    Free EMS memory may change as free XMS memory changes.

  Largest executable program size         569,024   (556K)
  Largest free upper memory block          22,160    (22K)
  MS-DOS is resident in the high memory area.



-------------------------
---------

Noilla muistim„„rill„ toimi hienosti!

Ihan perus VGA modessa, eli 13h :)

My”s ihan REAL MODE koodia, m„ tykk„„n Turbo Pascalista!

T„m„ on meid„n tuotos teid„n ( JUHLA V ) demo kilpailuun

Syy nykimiseen ja takkuiluun on ohjelmoijassa joka ei osaa eik„ jaksa
optimoida eik„ edes ohjelmoida. (itses„„li„???) 

Trouble shooting:

Blank screen - Try to get some more base memory

No sound - No soundcard

Disclaimer:

WE DO NOT TAKE ANY RESPONSIBLES ABOUT DAMAGES THAT THIS SOFTWARE CAN COUSE YOUR
HARDWARE! 


Credits for this production:
 Did what           Handle      Age     Real name

Code, design       : X-Regulus,  18,    Juuso Jokiniemi
fonts              : Yoshi    ,  18,    Nicklas ™sterholm
Music              : Dany     ,  19,    Daniel Kouvo      
Gfx                : Frey     ,  19,    Frey Mansikkaniemi

Contact info!

3G Design Official Homepage:
http://3gdesign.home.ml.org


Frey's homepage:
http://come.to/frey


U.S.S. Endeavour -  the whq of 3G Design!

