      +-------------------------------------------------------------------------
      |
      |      CENTRAL PROCESSING UNIT (CPU) 65816
      |
      +-------------------------------------------------------------------------
      |
      |  Related topics:
      |
      |   6510 instruction set
      |   6510 illegal instruction set
      |   6510 instruction chart
      |
      |   65816 instruction chart
      |
      |   6510/65816 Addressing modes
      |
      |  Instructions set:
      |
      |     BRA   Branch Always
      |     BRL   Branch Always Long
      |
      |     COP   Coprocessor
      |
      |     JML   Jump Long
      |     JSL   Jump Subroutine Long
      |
      |     MVN   Block Move Negative
      |     MVP   Block Move Positive
      |
      |     PEA   Push Effective Absolute Address on Stack (or Push Immediate Data on Stack)
      |     PEI   Push Effective Indirect Address on Stack
      |     PER   Push Effective Program Counter Relative Address on Stack
      |     PHB   Push Data Bank Register on Stack
      |     PHD   Push Direct Register on Stack
      |     PHK   Push Program Bank Register on Stack
      |     PHX   Push Index X on Stack
      |     PHY   Push index Y on Stack
      |     PLB   Pull Data Bank Register from Stack
      |     PLD   Pull Direct Register from Stack
      |     PLX   Pull Index X from Stack
      |     PLY   Pull Index Y form Stack
      |
      |     REP   Reset Status Bits
      |     RTL   Return from Subroutine Long
      |
      |     SEP   Set Processor Status Bits
      |     STP   Stop the Clock
      |     STZ   Store Zero in Memory
      |
      |     TCD   Transfer Accumulator to Direct Register
      |     TCS   Transfer Accumulator to Stack Pointer Register
      |     TDC   Transfer Direct Register to Accumulator
      |     TRB   Test and Reset Bit
      |     TSB   Test and Set Bit
      |     TSC   Transfer Stack Pointer Register to Accumulator
      |     TXY   Transfer Index X to Index Y
      |     TYX   Transfer Index Y to Index X
      |
      |     WAI   Wait for Interrupt
      |     WDM   Reserved for Future Expansion
      |
      |     XBA   Exchange AH and AL
      |     XCE   Exchange Carry and Emulation Bits
      |
      +-------------------------------------------------------------------------

       Back to Mainpage