     $DEDC/57052:   Set buffer pointer to side-sector

    Jump from $DED4, $DEEA, $E41E, $E46C:

    DEDC: 85 94     STA $94         ; printer lo
    DEDE: A6 82     LDX $82         ; channel number
    DEE0: B5 CD     LDA $CD,X       ; buffer number
    DEE2: AA        TAX
    DEE3: BD E0 FE  LDA $FEE0,X     ; buffer address hi
    DEE6: 85 95     STA $95         ; set
    DEE8: 60        RTS

        Previous Page / Next Page