     $C6CE/50894:   ?

    Jump from $ECF2:

    C6CE: A5 83     LDA $83
    C6D0: 48        PHA             ; secondary address and channel number
    C6D1: A5 82     LDA $82
    C6D3: 48        PHA
    C6D4: 20 DE C6  JSR $C6DE       ; create file entry for directory
    C6D7: 68        PLA
    C6D8: 85 82     STA $82
    C6DA: 68        PLA             ; get data back
    C6DB: 85 83     STA $83
    C6DD: 60        RTS

        Previous Page / Next Page