     $D4F6/54518:   Get byte from buffer

    Jump from $C5D1, $CF39, $CF40, $E00E, $E39F:

    D4F6: 85 71     STA $71         ; pointer lo
    D4F8: 20 93 DF  JSR $DF93       ; get buffer number
    D4FB: AA        TAX
    D4FC: BD E0 FE  LDA $FEE0,X     ; hi-byte buffer address
    D4FF: 85 72     STA $72         ; pointer hi
    D501: A0 00     LDY #$00
    D503: B1 71     LDA ($71),Y     ; get byte from buffer
    D505: 60        RTS

        Previous Page / Next Page