     $DEE9/57065:   Buffer pointer for side-sector

    Jump from $DD33, $DD57, $DF14, $E1FF, $E35A, $E3F4:

    DEE9: 48        PHA             ; pointer in side-sector
    DEEA: 20 DC DE  JSR $DEDC       ; set buffer pointer
    DEED: 48        PHA
    DEEE: 8A        TXA             ; buffer number
    DEEF: 0A        ASL             ; times 2
    DEF0: AA        TAX
    DEF1: 68        PLA
    DEF2: 95 9A     STA $9A,X       ; buffer pointer hi
    DEF4: 68        PLA
    DEF5: 95 99     STA $99,X       ; buffer pointer lo
    DEF7: 60        RTS

        Previous Page / Next Page