The MOS 6567/6569 video controller (VIC-II) and its application in the Commodore 64
Contents 3. Description of the VIC
3.3. Color palette |
The VIC has a hard-wired palette of 16 colors that are encoded with 4 bits:
| 0 |  | black |  | 4 |  | pink |  | 8 |  | orange |  | 12 |  | medium gray
| 1 |  | white |  | 5 |  | green |  | 9 |  | brown |  | 13 |  | light green
| 2 |  | red |  | 6 |  | blue |  | 10 |  | light red |  | 14 |  | light blue
| 3 |  | cyan |  | 7 |  | yellow |  | 11 |  | dark gray |  | 15 |  | light gray