     $C806/51206:   Print 'blocks free.'

    Jump from $C6F2, $C707:

    C806: 20 AC C7  JSR $C7AC       ; erase buffer
    C809: A0 0B     LDY #$0B        ; 12 characters

    Jump from $C812:

    C80B: B9 17 C8  LDA $C817,Y     ; 'blocks free.'
    C80E: 99 B1 02  STA $02B1,Y     ; write in buffer
    C811: 88        DEY
    C812: 10 F7     BPL $C80B
    C814: 4C 4D EF  JMP $EF4D       ; number of free blocks in front

        Previous Page / Next Page