     $D44D/54349:   Read next block

    Jump from $C629, $C8B0, $EE07:

    D44D: 20 93 DF  JSR $DF93       ; get buffer number
    D450: 0A        ASL             ; times 2
    D451: AA        TAX
    D452: A9 00     LDA #$00
    D454: 95 99     STA $99,X       ; buffer pointer to zero
    D456: A1 99     LDA ($99,X)     ; get first byte from buffer
    D458: F0 05     BEQ $D45F       ; no block following?
    D45A: D6 99     DEC $99,X       ; buffer pointer to -1
    D45C: 4C 56 D1  JMP $D156       ; read next block

    Jump from $D458:

    D45F: 60        RTS

        Previous Page / Next Page