     $DDFD/56829:   Write bytes for following track

    Jump from $E3AC, $E3BF:

    DDFD: 20 2B DE  JSR $DE2B       ; set buffer pointer
    DE00: A5 80     LDA $80         ; track number
    DE02: 91 94     STA ($94),Y     ; in buffer
    DE04: C8        INY
    DE05: A5 81     LDA $81         ; sector number
    DE07: 91 94     STA ($94),Y     ; in buffer
    DE09: 4C 05 E1  JMP $E105       ; set rel-flag

        Previous Page / Next Page