     $DE95/56981:   Get following track and sector from buffer

    Jump from $DA34, $E03F, $E06B:

    DE95: A9 00     LDA #$00
    DE97: 20 C8 D4  JSR $D4C8       ; buffer pointer to zero
    DE9A: 20 37 D1  JSR $D137       ; get byte
    DE9D: 85 80     STA $80         ; save as track
    DE9F: 20 37 D1  JSR $D137       ; get byte
    DEA2: 85 81     STA $81         ; as sector
    DEA4: 60        RTS

        Previous Page / Next Page