     $DE19/56857:   Following track for last block

    Jump from $DD7E, $E3D1:

    DE19: 20 2B DE  JSR $DE2B       ; set buffer pointer
    DE1C: A9 00     LDA #$00        ; zero
    DE1E: 91 94     STA ($94),Y     ; as track number
    DE20: C8        INY
    DE21: A6 82     LDX $82         ; channel number
    DE23: B5 C1     LDA $C1,X       ; pointer in block
    DE25: AA        TAX
    DE26: CA        DEX             ; minus 1
    DE27: 8A        TXA
    DE28: 91 94     STA ($94),Y     ; as pointer in block
    DE2A: 60        RTS

        Previous Page / Next Page