     $D7B4/55220:   OPEN command, secondary addr 15

    Jump from $C15D:

    D7B4: A5 83     LDA $83         ; secondary address
    D7B6: 8D 4C 02  STA $024C
    D7B9: 20 B3 C2  JSR $C2B3       ; get line length, erase flags
    D7BC: 8E 2A 02  STX $022A
    D7BF: AE 00 02  LDX $0200       ; first character from buffer
    D7C2: AD 4C 02  LDA $024C       ; secondary address
    D7C5: D0 2C     BNE $D7F3       ; not equal 0 (LOAD)?

        Previous Page / Next Page