     $CEED/52973:   Add 3-byte registers

    Jump from $CE54, $CEA3:

    CEED: 18        CLC
    CEEE: A2 FD     LDX #$FD

    Jump from $CEF7:

    CEF0: B5 8E     LDA $8E,X       ; register $90/$91/$92
    CEF2: 75 93     ADC $93,X       ; add to register $8B/$8C/$8D
    CEF4: 95 8E     STA $8E,X
    CEF6: E8        INX
    CEF7: D0 F7     BNE $CEF0
    CEF9: 60        RTS

        Previous Page / Next Page