     $DE2B/56875:   buffer pointer to zero

    Jump from $DDFD, $DE0C, $DE19, $E1B2, $E2E2:

    DE2B: 20 93 DF  JSR $DF93       ; get buffer number
    DE2E: 0A        ASL             ; times 2
    DE2F: AA        TAX
    DE30: B5 9A     LDA $9A,X       ; buffer pointer hi
    DE32: 85 95     STA $95
    DE34: A9 00     LDA #$00
    DE36: 85 94     STA $94         ; buffer pointer lo
    DE38: A0 00     LDY #$00
    DE3A: 60        RTS

        Previous Page / Next Page