     $DD8D/56717:   Write byte in side-sector block

    Jump from $DD38, $DD3D, $DD42, $DD48, $DD4D, $DD52, $DD5F, $DD64, $E3FA,
              $E3FE:

    DD8D: 48        PHA             ; save byte
    DD8E: A6 82     LDX $82         ; channel number
    DD90: B5 CD     LDA $CD,X       ; buffer number of the side-sector
    DD92: 4C FD CF  JMP $CFFD       ; write byte in buffer

        Previous Page / Next Page