     $DE0C/56844:   Get following track and sector numbers

    Jump from $E2AD, $E3D7:

    DE0C: 20 2B DE  JSR $DE2B       ; set buffer pointer
    DE0F: B1 94     LDA ($94),Y     ; following track number
    DE11: 85 80     STA $80
    DE13: C8        INY
    DE14: B1 94     LDA ($94),Y     ; and get sector number
    DE16: 85 81     STA $81
    DE18: 60        RTS

        Previous Page / Next Page