     $D475/54389:   Allocate buffer and read block

    Jump from $C5C1, $C60E, $C880, $CA0C, $EDEB:

    D475: A9 01     LDA #$01

    Jump from $E7D5:

    D477: 8D 4A 02  STA $024A       ; file type to sequential
    D47A: A9 11     LDA #$11        ; 17
    D47C: 85 83     STA $83         ; secondary address
    D47E: 20 46 DC  JSR $DC46       ; allocate buffer and read block
    D481: A9 02     LDA #$02
    D483: 4C C8 D4  JMP $D4C8       ; buffer pointer to 2

        Previous Page / Next Page