      +------------------------------------------------------------------------
      |
      |      SUPERCPU - REGISTER DESCRIPTIONS
      |
      +------------------------------------------------------------------------
      |
      |   $D074/53364/SCPU+4        GEOS Optimization
      |   $D075/53365/SCPU+5        VIC Bank 01 Optimization
      |   $D076/53366/SCPU+6        BASIC Optimization
      |   $D077/53367/SCPU+7        No Optimization (V1: Default)
      |   $D079/53369/SCPU+9        Duplicate: Speed Select - Turbo (20 MHz)
      |   $D07A/53370/SCPU+10       Speed Select - Normal (1 MHz)
      |   $D07B/53371/SCPU+11       Speed Select - Turbo (20 MHz)
      |   $D07D/53373/SCPU+13       Duplicate: Hardware Register Disable
      |   $D07E/53374/SCPU+14       Hardware Register Enable
      |   $D07F/53375/SCPU+15       Hardware Register Disable
      |
      |   $D0B0/53424/SCPU+64       SuperCPU Mode Detect Register
      |   $D0B2/53426/SCPU+66       Hardware Register-/System Flag
      |   $D0B3/53427/SCPU+67       Enhanced Optimization Register (V2 only!)
      |   $D0B4/53428/SCPU+68       Optimization Mode Flags
      |   $D0B5/53429/SCPU+69       JiffyDOS-/Speed Switch Flag
      |   $D0B6/53430/SCPU+70       Processor Emulation-/Reset Flag
      |   $D0B8/53432/SCPU+72       Software 1 MHz-/Master 1Mhz Flag
      |   $D0BC/53433/SCPU+76       DOS Extension-/RAMLink Hardware Reg. Flag
      |
      |
      |   $D200-$D2FF/53760-54015   System-RAM:
      |   $D27B/53883/SCPURAM+123    SIMM-Type
      |   $D27C/53884/SCPURAM+124    First Available Page of SuperRAM
      |   $D27D/53885/SCPURAM+125    Bank of First Available Page of SuperRAM
      |   $D27E/53886/SCPURAM+126    Last Available Page of SuperRAM + 1
      |   $D27F/53887/SCPURAM+127    Bank of Last Available Page of SuperRAM + 1
      |
      |   $D300-$D3FF/54016-54271   User-RAM
      |
      +------------------------------------------------------------------------

       Back to Mainpage