     $DEA5/56997:   Copy buffer contents

    Jump from $E467:

    DEA5: 48        PHA
    DEA6: A9 00     LDA #$00
    DEA8: 85 6F     STA $6F
    DEAA: 85 71     STA $71
    DEAC: B9 E0 FE  LDA $FEE0,Y     ; buffer address Y, hi
    DEAF: 85 70     STA $70
    DEB1: BD E0 FE  LDA $FEE0,X     ; buffer address X, lo
    DEB4: 85 72     STA $72
    DEB6: 68        PLA
    DEB7: A8        TAY
    DEB8: 88        DEY

    Jump from $DEBE:

    DEB9: B1 6F     LDA ($6F),Y
    DEBB: 91 71     STA ($71),Y
    DEBD: 88        DEY
    DEBE: 10 F9     BPL $DEB9
    DEC0: 60        RTS

        Previous Page / Next Page