     $ED59/60761:   Transmit dir line

    Jump from $ECD9, $ED03, $ED2F:

    ED59: A0 00     LDY #$00

    Jump from $ED64:

    ED5B: B9 B1 02  LDA $02B1,Y     ; character from buffer
    ED5E: 20 F1 CF  JSR $CFF1       ; write in output buffer
    ED61: C8        INY
    ED62: C0 1B     CPY #$1B        ; 27 characters?
    ED64: D0 F5     BNE $ED5B
    ED66: 60        RTS

        Previous Page / Next Page